0A07-01#sh spanning-tree 
 STP 0 
 Vlan 1,10,11,99
  Spanning Tree enabled protocol ieee 802.1w (Rapid Spanning-Tree)
  Root ID    Priority     0
             Address      00:a0:c8:8c:13:90
             The root of the spanning tree
             Hello Time   2 sec  Max Age 20 sec  Forward Delay 15 sec

  Bridge ID  Priority     0
             Address      00:a0:c8:8c:13:90
             Aging Time   300

Interface        Role Sts Cost      Prio.Nbr Type 
---------------- ---- --- --------- -------- ------------------------------
giga-swx 0/2     Desg FWD 4          128.26  P2p   
giga-swx 0/3     Desg FWD 4          128.27  P2p   
giga-swx 0/4     Desg FWD 4          128.28  Edge P2p

======================================================

0A07-02#sh span
 STP 0 
 Vlan 1,10,99
  Spanning Tree enabled protocol ieee 802.1w (Rapid Spanning-Tree)
  Root ID    Priority     0
             Address      00:a0:c8:8c:13:90
             Cost         4
             Port         52 (giga-swx 0/4)
             Hello Time   2 sec  Max Age 20 sec  Forward Delay 15 sec

  Bridge ID  Priority     32768
             Address      00:a0:c8:8d:90:05
             Aging Time   300

Interface        Role Sts Cost      Prio.Nbr Type 
---------------- ---- --- --------- -------- ------------------------------
swx 0/37         Desg FWD 19         128.37  Edge P2p
giga-swx 0/1     Desg FWD 4          128.49  Edge P2p
giga-swx 0/3     Desg FWD 4          128.51  P2p   
giga-swx 0/4     Root FWD 4          128.52  P2p   

======================================================

0A07-03#sh span
 STP 0 
 Vlan 1,10,99
  Spanning Tree enabled protocol ieee 802.1w (Rapid Spanning-Tree)
  Root ID    Priority     0
             Address      00:a0:c8:8c:13:90
             Cost         8
             Port         52 (giga-swx 0/4)
             Hello Time   2 sec  Max Age 20 sec  Forward Delay 15 sec

  Bridge ID  Priority     1
             Address      00:a0:c8:8d:91:ad
             Aging Time   300

Interface        Role Sts Cost      Prio.Nbr Type 
---------------- ---- --- --------- -------- ------------------------------
giga-swx 0/1     Desg FWD 4          128.49  Edge P2p
giga-swx 0/3     Desg FWD 4          128.51  P2p   
giga-swx 0/4     Root FWD 4          128.52  P2p   

======================================================

0E19-01#sh span
 STP 0 
 Vlan 1,11,99
  Spanning Tree enabled protocol ieee 802.1w (Rapid Spanning-Tree)
  Root ID    Priority     0
             Address      00:a0:c8:8c:13:90
             Cost         4
             Port         52 (giga-swx 0/4)
             Hello Time   2 sec  Max Age 20 sec  Forward Delay 15 sec

  Bridge ID  Priority     32768
             Address      00:a0:c8:8d:92:17
             Aging Time   300

Interface        Role Sts Cost      Prio.Nbr Type 
---------------- ---- --- --------- -------- ------------------------------
giga-swx 0/3     Desg FWD 4          128.51  P2p   
giga-swx 0/4     Root FWD 4          128.52  P2p   

======================================================

0E19-02#sh spanning-tree 
 STP 0 
 Vlan 1,11,99
  Spanning Tree enabled protocol ieee 802.1w (Rapid Spanning-Tree)
  Root ID    Priority     0
             Address      00:a0:c8:8c:13:90
             Cost         8
             Port         52 (giga-swx 0/4)
             Hello Time   2 sec  Max Age 20 sec  Forward Delay 15 sec

  Bridge ID  Priority     32768
             Address      00:a0:c8:7e:6e:60
             Aging Time   300

Interface        Role Sts Cost      Prio.Nbr Type 
---------------- ---- --- --------- -------- ------------------------------
giga-swx 0/3     Desg FWD 4          128.51  P2p   
giga-swx 0/4     Root FWD 4          128.52  P2p   

======================================================

0E19-03#sh span
 STP 0
 Vlan 1,11,99
  Spanning Tree enabled protocol ieee 802.1w (Rapid Spanning-Tree)
  Root ID    Priority     0
             Address      00:a0:c8:8c:13:90
             Cost         12
             Port         51 (giga-swx 0/3)
             Hello Time   2 sec  Max Age 20 sec  Forward Delay 15 sec

  Bridge ID  Priority     32768
             Address      00:a0:c8:7e:64:70
             Aging Time   300

Interface        Role Sts Cost      Prio.Nbr Type
---------------- ---- --- --------- -------- ------------------------------
giga-swx 0/3     Root FWD 4          128.51  P2p
giga-swx 0/4     Altn BLK 4          128.52  P2p