NV6247#
NV6247#sho ver
ADTRAN, Inc. OS version R10.8.0.E
  Mainline Version: ENM.13.39
  Checksum: AA5BBFAA
  Built on: Tue May 21 16:57:02 2013
  Upgrade key: d9e58c34a0caafea29aac7ea351f4397
Hardware version D.5
Boot ROM version A5.01.00
  Checksum: 916B
  Built on: Fri Sep 09 11:32:41 2011
Copyright (c) 1999-2013, ADTRAN, Inc.
Platform: NetVanta 6247, part number 4740207G21
Serial number CFG1147590
Flash: 138412032 bytes  DRAM: 134217727 bytes

NV6247 uptime is 0 days, 3 hours, 24 minutes, 1 seconds

slot 0, DSP 1
  DSP software version: A5.01.00
  DSP hardware version: TI Dsp C266X
  Total channels: 30

slot 0, DSP 2
  DSP software version: A5.01.00
  DSP hardware version: TI Dsp C266X
  Total channels: 30

System returned to ROM by Power On Reset
Current system image file is "NV6200A-R10-8-0-E.biz"
Primary boot system image file is "NV6200A-R10-8-0-E.biz"
Backup boot system image file is "9700204-20A501.biz"
Primary system configuration file is "startup-config"
NV6247#
NV6247#
NV6247#sho ip ro
Codes: C - connected, S - static, R - RIP, O - OSPF, B - BGP
       E1 - OSPF external type 1, E2 - OSPF external type 2
       IA - OSPF inter area

Gateway of last resort is 198.162.0.34 eth 0/2

O E2 0.0.0.0/0 [110/10/1] via 198.162.0.34, eth 0/2
C    10.0.0.0/24 is directly connected, tunnel 1
C    198.162.0.8/29 is directly connected, eth 0/1
O    198.162.0.24/29 [110/0/2] via 198.162.0.34, eth 0/2
C    198.162.0.32/29 is directly connected, eth 0/2

NV6247#
NV6247#
NV6247#sho ip mr
IP Multicast Routing Table
Flags:  S - Sparse, C - Connected, P - Pruned, J - Join SPT, T - SPT-bit Set,
F - Register, R - RP-bit Set
Timers: Uptime/Expires

(*, 224.4.4.1), 03:23:35/stopped , RP 0.0.0.0, Flags:
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    eth 0/1, Forward, 03:23:29/00:00:00
    eth 0/2, Forward, 02:45:28/00:02:38

(*, 224.4.4.2), 03:23:35/stopped , RP 0.0.0.0, Flags:
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    eth 0/1, Forward, 03:23:29/00:00:00
    eth 0/2, Forward, 02:45:32/00:02:57

(*, 239.255.255.250), 02:45:26/00:03:04, RP 198.162.0.10, Flags: SJ
  Incoming interface: Null, RPF nbr 0.0.0.0
  Outgoing interface list:
    eth 0/2, Forward, 02:45:26/00:03:04

NV6247#
NV6247#
NV6247#sho igmp gr
% Unrecognized command
NV6247#sho ip igmp gr
IGMP Connected Group Membership
Group Address    Interface                Uptime    Expires   Last Reporter
NV6247#
NV6247#
NV6247#sho ip igmp int
Loopback is UP
  IP Address is 127.0.0.1, netmask is 255.255.255.255
  IGMP is disabled on interface
null 0 is UP
  IP Address is 127.0.0.2, netmask is 255.255.255.255
  IGMP is disabled on interface
eth 0/1 is UP
  IP Address is 198.162.0.10, netmask is 255.255.255.248
  IGMP is enabled on interface
  Current IGMP version is 2
  IGMP query interval is 60 seconds
  IGMP querier timeout is 120 seconds
  IGMP max query response time is 10 seconds
  Last member query count is 2
  Last member query response interval is 1000 ms
  IGMP activity: 131 joins, 2 leaves
  IGMP querying router is 198.162.0.10
  IGMP helper address is disabled
eth 0/2 is UP
  IP Address is 198.162.0.33, netmask is 255.255.255.248
  IGMP is enabled on interface
  Current IGMP version is 2
  IGMP query interval is 60 seconds
  IGMP querier timeout is 120 seconds
  IGMP max query response time is 10 seconds
  Last member query count is 2
  Last member query response interval is 1000 ms
  IGMP activity: 0 joins, 0 leaves
  IGMP querying router is 198.162.0.33
  IGMP helper address is disabled
tunnel 1 is UP
  IP Address is 10.0.0.1, netmask is 255.255.255.0
  IGMP is disabled on interface
NV6247#
NV6247#
NV6247#sho pim nei
% Unrecognized command
NV6247#sho ip pim nei
Port                 Neighbor        Holdtime(sec)   Age(sec) Uptime(sec)
-------------------- --------------- ------------- ---------- -----------
eth 0/2              198.162.0.34              105          8       12217
NV6247#
NV6247#
NV6247#sho pim stat
% Unrecognized command
NV6247#sho ip pim stat
PIM-SM State Table
Flags:  S - Sparse, C - Connected, P - Pruned, J - Join SPT, T - SPT-bit Set,
F - Register, R - RP-bit Set
Timers: Uptime/Expires

(*, 224.4.4.1), 02:48:15/00:02:40, RP 198.162.0.10, Flags: SJ
  Forwarding Entry: Yes
  Incoming interface: Null, RPF nbr 0.0.0.0
  Upstream Join/Prune State: Joined
  Register State: No Info
  RegStop Timer (sec): stopped
  Join/Prune Timer (sec): 44
  Override Timer (sec): stopped
  Multicast Border Router: 0.0.0.0
  Packets Forwarded: 0
  Outgoing interface list:
    eth 0/2, Forward, 02:46:26/00:02:40
      Downstream Join/Prune State: Join
      Assert Winner State: No Info
      Assert Timer (sec): stopped
      Assert Winner: 0.0.0.0
      Assert Winner Metric: infinity
      Local Membership: No
      Forwarding State: Forwarding
  Inherited output list:  Null

(*, 224.4.4.2), 02:48:15/00:02:59, RP 198.162.0.10, Flags: SJ
  Forwarding Entry: Yes
  Incoming interface: Null, RPF nbr 0.0.0.0
  Upstream Join/Prune State: Joined
  Register State: No Info
  RegStop Timer (sec): stopped
  Join/Prune Timer (sec): 44
  Override Timer (sec): stopped
  Multicast Border Router: 0.0.0.0
  Packets Forwarded: 0
  Outgoing interface list:
    eth 0/2, Forward, 02:46:30/00:02:59
      Downstream Join/Prune State: Join
      Assert Winner State: No Info
      Assert Timer (sec): stopped
      Assert Winner: 0.0.0.0
      Assert Winner Metric: infinity
      Local Membership: No
      Forwarding State: Forwarding
  Inherited output list:  Null

(*, 239.255.255.250), 02:46:24/00:03:06, RP 198.162.0.10, Flags: SJ
  Forwarding Entry: Yes
  Incoming interface: Null, RPF nbr 0.0.0.0
  Upstream Join/Prune State: Joined
  Register State: No Info
  RegStop Timer (sec): stopped
  Join/Prune Timer (sec): 36
  Override Timer (sec): stopped
  Multicast Border Router: 0.0.0.0
  Packets Forwarded: 0
  Outgoing interface list:
    eth 0/2, Forward, 02:46:24/00:03:06
      Downstream Join/Prune State: Join
      Assert Winner State: No Info
      Assert Timer (sec): stopped
      Assert Winner: 0.0.0.0
      Assert Winner Metric: infinity
      Local Membership: No
      Forwarding State: Forwarding
  Inherited output list:  Null
NV6247#
NV6247#debug ip igmp
NV6247#debug ip mr
NV6247#06:45:14: IGMP: sent General Query on eth 0/2
06:45:14: IGMP: sent General Query on eth 0/1

0/2 is not configured06:46:14: IGMP: sent General Query on eth 0/2
06:46:14: IGMP: sent General Query on eth 0/1

0/2 is not configured06:47:14: IGMP: sent General Query on eth 0/2
06:47:14: IGMP: sent General Query on eth 0/1

0/2 is not configured06:48:14: IGMP: sent General Query on eth 0/2
06:48:14: IGMP: sent General Query on eth 0/1
06:49:14: IGMP: sent General Query on eth 0/2
06:49:14: IGMP: sent General Query on eth 0/1
06:50:14: IGMP: sent General Query on eth 0/2
06:50:14: IGMP: sent General Query on eth 0/1

0/2 is not configured06:51:14: IGMP: sent General Query on eth 0/2
06:51:14: IGMP: sent General Query on eth 0/1

0/2 is not configured06:52:14: IGMP: sent General Query on eth 0/2
06:52:14: IGMP: sent General Query on eth 0/1

0/2 is not configured06:53:14: IGMP: sent General Query on eth 0/2
06:53:14: IGMP: sent General Query on eth 0/1
06:54:14: IGMP: sent General Query on eth 0/2
06:54:14: IGMP: sent General Query on eth 0/1
06:55:14: IGMP: sent General Query on eth 0/2
06:55:14: IGMP: sent General Query on eth 0/1